ONE SET OF MTR'S ARE TO BE EMAILED TO THE OMAHA NUMBER LISTED ABOVE. 
PIPE WILL BE MANUFACTURED IN ACCORDANCE WITH API 5L PSL 2 45TH OR 46TH EDITION, DOUBLE RANDOM LENGTHS. 
J D FIELDS & CO. WILL STENCIL EACH JOINT OF PIPE, WITH THE PROPER HEAT NUMBER, NNG PURCHASE ORDER NUMBER AND WORK ORDER NUMBER. 
ALL PERTINENT INDENTIFYING INFORMATION MUST BE TRANSFERED TO THE I.D. OF EACH JOINT OF PIPE.
NOTE: TRUCK TRANSPORTATION IS ESTIMATED TO BE 24 HRS. TRUCKERS CONTACT LES FREDRICK @402-681-8353 AT LEAST 24 HOURS PRIOR TO DELIVERY.
SHIP TO: NORTHERN NATURAL GAS COMPANY
              145 F ROAD
               MACKSVILLE, KANSAS 67557
              ATTN: LES FREDRICK – CHIEF INSPECTOR
              PH: 402-681-8353 (CELL)

CONSTRUCTION COORDINATOR: TBD 
Northern Natural Gas Pipe Loading Requirements Pipe shipments that do not satisfy the following criteria or standards will, at the sole discretion of Northern, be rejected or made subject to special unloading requirements at the expense of the shipper or supplier. 
• Pipe that is designated to be loaded and delivered to a Northern location shall be tier loaded, never bundled or pyramid loaded. Overall height of the tiers, including dunnage, shall not exceed 84-inches. 
• Loads must be tied down with non-metallic straps. Each tier shall have its own tie-down straps. The shipment shall be free from any visual signs of coating or material damage including visual signs of fatigue cracking. 
• Inbound pipe shipments to all Northern locations, must be tiered with 4-inch-by-4-inch hardwood dunnage material to maintain sufficient spacing to allow forks from a lift underneath the pipe during unloading. 
• Hardwood dunnage shall be bare wood that is free of nails or other objects that could damage pipe or coating. 
• Hardwood dunnage shall not be stacked between tiers. 
• Hardwood dunnage shall have pipe chocks sufficiently fastened at each end to prevent movement of the pipe. Pipe chocks shall meet the minimum standards set forth in the attachment. 
• Pipe chocks must be properly positioned to ensure the centerline of the outer pipe placed on each ascending tier does not cross the centerline of the outer pipe below. See attachment. 
*************************************************************************************ATTENTION - PRIORITY
ALL MATERIAL ON THIS PURCHASE ORDER MUST BE IN COMPLIANCE WITH THE NORTHERN NATURAL GAS APPROVED MANUFACTURERS LIST. ALL COSTS AND DAMAGES ASSOCIATED WITH NON-COMPLIANCE MATERIAL WILL BE CHARGED BACK TO SUPPLIER. *************************************************************************************PIPE DOCUMENTATION, MTR'S, SHIPPING 
THE HEAT NUMBERS AND PURCHASE ORDER NUMBER FOR ALL PIPE SHIPPED UNDER A PURCHASE ORDER SHALL BE SHOWN ON ALL SHIPPING NOTICES AND MILL TEST REPORTS (MTR'S). 
MTR'S ARE REQUIRED FOR ALL STEEL PIPE EXCEPT PIPE SPECIFIED FOR NON-HAZARDOUS SERVICE, SUCH AS INSTRUMENT AIR AND POTABLE WATER AT PRESSURES + / - 60 PSIG AND TEMPERATURES BETWEEN 40 DEGREES F AND 130 DEGREES F. PURCHASE ORDER
MTR'S ARE TO BE FURNISHED WITH THE APPLICABLE HEAT NUMBER(S) AND PURCHASE DOCUMENT NUMBER(S) SHOWN ON EACH PAGE. MTR'S ARE TO BE FURNISHED IN TRIPLICATE, ONE SET WILL BE SENT WITH THE PIPE AND TWO SETS WILL BE SENT TO THE BUYER. FAILURE TO COMPLY WITH REQUESTS WILL DELAY PAYMENT OF THE INVOICE. 

FOR PIPE 2 INCHES UP TO 12 INCHES NOMINAL PIPE SIZE (NPS), THE INFORMATION LISTED BELOW SHOULD BE PAINT STENCILED ON THE OUTSIDE SURFACE OF BOTH ENDS OF EACH PIECE. PIPE LARGER THAN 12 INCHES NPS SHOULD BE MARKED ON THE INSIDE SURFACE OF BOTH ENDS OF EACH PIECE OF PIPE. THE SIZE BREAK FOR MARKING IS 12 INCHES NPS FOR PIPE SPECIFIED TO NNG STANDARD 4905. 
FOR PIPE 1.9 INCHES O.D. AND SMALLER, THE INFORMATION CAN BE DIE STAMPED ON A METAL TAG FIXED TO THE BUNDLE. DIE STAMPING OF THE PIPE IS NOT PERMITTED. 
THIS INFORMATION SHALL BE IN ACCORDANCE WITH THE APPLICABLE PIPE SPECIFICATION API5L OR ASTM A 106. MARKINGS SHALL INCLUDE AT LEAST: 
1. MANUFACTURER'S NAME OR MARK ON API 5L AND ASTM A 106 
2. API OR ASTM SPECIFICATION ON SPEC 5L AND ASTM A 106 
3. OUTSIDE DIAMETER OR NPS ON API 5L ONLY 
4. WALL THICKNESS, MUST BE INCLUDED FOR API 5L (*) AND PER SCHEDULE FOR ASTM A 106 
5. WEIGHT PER FOOT - SIZES NPS 2 AND LARGER ON API 5L AND ASTM A 106 6. GRADE ON API 5L AND ASTM A 106 
7. PROCESS OF MANUFACTURER ON API 5L AND ASTM A 106 
8. HEAT TREATMENT, IF APPLICABLE ON API 5L AND ASTM A 106 
9. MILL TEST PRESSURE ON API 5L AND ASTM A 106 
10. LENGTH OF JOINT (+ / - 1-1/2 IN. NPS) ON API 5L AND ASTM A 106 
11. HEAT NUMBER (*) 12. PURCHASER'S DOCUMENT NUMBER (*) 
13. SUPPLEMENTARY REQIREMENTS, IF APPLICABLE (*) 
(*) MARKINGS ARE NOT REQUIRED BY MANUFACTURING SPECIFICATIONS BUT MUST BE INCLUDED. 
PIPE SHIPMENTS INBOUND FROM SUPPLIER LOCATONS MUST BE STACKED WITH 4 IN X 4 IN HARDWOOD DUNNAGE OR EQUIVALENT MATERIAL. THIS WILL INSURE SUFFICENT SPACING TO ALLOW FORKS FROM A LIFT UNDERNEATH THE PIPE DURING LOADING AND UNLOADING. DUNNAGE MATERIAL MUST HAVE SUPPORTS OR CHOCKS SUFFICIENTLY FASTENED AT EACH END TO PREVENT MOVEMENT OF THE PIPE. 
PIPE SHIPMENTS THAT DO NOT SATISFY THESE CRITERIA OR STANDARDS MAY, AT THE SOLE DISCRETION OF THE COMPANY, BE REJECTED OR MADE SUBJECT TO SPECIAL UNLOADING REQUIREMENTS AT THE EXPENSE OF THE SHIPPER OR SUPPLIER. 
ATTACHED NORTHERN NATURAL GAS COMPANY TERMS AND CONDITIONS WILL GOVERN THIS PURCHASE ORDER.
